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	[bookmark: _Toc89994933][bookmark: _Toc225764775]Document and Section Affected: Handbook Section III Building code, Section F. 2, c-e

	Requested Change(s) (list paragraph, page, line, and change):  
From: 2 c. Uncovered front stoops and decks may extend up to six (6) feet into the thirty (30) foot setback required at the front of the Lot with a maximum of (48) square feet allowed. Steps are not included in setback restrictions in the front or rear of house; however, step landings “between stair runs” are included. The maximum size of a landing can be forty-eight (48) sq. feet, and a maximum length of eight (8) feet when they fall within front and rear set back area. If steps and landing fall inside the ten (10) foot setback, then the maximum size of landing is twenty-four (24) square feet with a maximum of four feet into the 10-foot setback restriction for both steps and landing.  To be considered a landing there must be a minimum of a seven inch drop from the main deck. Elevated walkways between landings or landing and rear decks are permitted and may not exceed four feet into the side yard setbacks. 
d. Uncovered (open) attached rear decks, which may extend 10’ into the rear setback.   
e. Ground level decks (less than 1’ tall) and walks may be built to the lot line

To:
2 c. Uncovered front stoops and decks may extend up to eight (8’) feet into the thirty (30) foot setback required at the front of the Lot with a maximum of (240) square feet allowed.
d. Steps are not included in setback restrictions in the front or rear of house; however, step landings “between stair runs” are included. The maximum size of a landing can be forty-eight (48) sq. feet, and a maximum length of eight (8) feet when they fall within front and rear set back area.
e. For rear uncovered decks, if steps and landing fall inside the ten (10) foot setback, then the maximum size of landing is twenty-four (24) square feet with a maximum of four feet into the 10-foot setback restriction for both steps and landing.  To be considered a landing there must be a minimum of a seven-inch drop from main deck.
f. Elevated walkways between landings or landing and rear decks are permitted and may not exceed four feet into the side yard setbacks. 
g. Uncovered (open) attached rear decks, which may extend 10’ into the rear setback.    
h. Ground level decks (less than 1’ tall) and walks may be built to the lot line
 

	Justification:  Why is this change needed?  
Because appeals have already been given to accommodate these front decks/stoops.

	Impacts:  If not approved, what are the consequences?  
More unnecessary appeals 

	Appropriate Committee:     Approve ____  Disapprove: ____      N/A:__X__     Date:

	Recommendations for the Board:


	Approval Status:     Approved: _X_  Disapproved: ____          Date:  11-17-22

	Board Comments:
Approved as recorded at the 11-17-22 BOD Meeting
Updated Handbook:  11-23-22 (jjp)




