	BEAVER LAKE ASSOCIATION

DOCUMENT CONTROL FORM

	Requester:  Building Inspector
	Ctrl Number:   092
	Date 02/22/06

	Document and Section Affected: Beaver Lake Building Code, Section III



	Requested Change(s) (list paragraph, page, line, and change):  

Paragraph P.6.c, change to read:

“c.  Only American Society of Mechanical Engineers (ASME) approved containers constructed for underground service and marked accordingly can be installed underground.  The placement of Anode Bags close to the tank is highly recommended for underground tanks to prevent corrosion.  Department Of Transportation (DOT) cylinders must be installed above ground.  Governing rules are the National Propane Gas Association (NPGA) # 412-94 and the National Fire Protection Association (NFPA)-58.  The tank must be inspected by the Building Inspector prior to installation.  



	Justification:  Why is this change needed?

Our current codes don’t state that there is a special type of tank needed for underground placement.

	Impacts:  If not approved, what are the consequences?

Someone could install a tank not suited for underground placement.



	Appropriate Committee:   None  Req  Approve __Disapprove: __N/A:  Date:   

	Recommendations for the Board:

 Change wording and include the NPGA #412-94 where the regulation can be found.


	Approval Status:     Approved: __X__  Disapproved: ____          Date:  20 Apr 06

	Board Comments:
18 Apr 06:  Approved at working session

20 Apr 06:  Approved at Board meeting




P.
TANKS


1.
A Beaver Lake Building Permit XE "building permit"  is required for installation of a Tank XE "tanks" .


2.
Tanks XE "tanks"  shall not be permitted within fifty (50) feet of the Lake.


3.
Tanks XE "tanks"  shall not be placed on a Lot which is not improved with a Dwelling XE "dwelling" , Commercial XE "commercial"  Building or Mobile Home XE "mobile home" .


4.
Above-ground Tanks XE "tanks"  located on a Residential XE "residential"  Lot, Equestrian XE "equestrian"  Lot, Mobile Home XE "mobile home"  Lot, or Commercial XE "commercial"  Lot shall be screened from view by shrubbery XE "shrubbery"  or a solid wood or plastic fence XE "fence" .  Chain link fences XE "fences"  are not permitted to screen a Tank.  If wood or plastic lattice is used to screen a Tank, the holes in such lattice may not exceed one inch (1) inch square (one and one-half (1½) inches when measured diagonally.   Shrubbery used to screen a Tank shall be of the evergreen family and shall be large and dense enough when planted to completely shield the Tank from view.  In screening a Tank, consideration should be given to proper ventilation and access for refilling and repair XE "repair" .


5.
Tanks XE "tanks"  shall be located on the side or back yard of Lot if at all possible provided; however, that a Tank installed on a corner Lot shall be located in the back yard of the Lot.  Lakefront XE "lakefront"  lots shall not place tank within 50 feet of water's edge.  If Tank has to be located in the front yard (roadside) to meet setbacks, it must be placed at least fifteen (15) feet inside the front property line.


6.
The following requirements apply to Tanks XE "tanks"  buried or to be buried on any Lot:



a.
The application XE "application"  for a Beaver Lake Building Permit XE "building permit"  must include a plot plan XE "plot plan"  showing the proposed location of the Tank XE "tanks"  on the Lot and filed with the Beaver Lake Association XE "Association" .



b.
The location of the Tank XE "tanks"  on the Lot shall comply with the setback XE "setback"  requirements contained in the Covenants XE "Covenants"  and Restrictions.

Change:

c.
The Tank XE "tanks"  must be inspected by the Building Inspector XE "Building Inspector"  prior to installation.  The Building Inspector shall supervise the installation of the Tank.

To Read:   c.  Only American Society of Mechanical Engineers (ASME) approved containers constructed for underground service and marked accordingly can be installed underground.  Department Of Transportation (DOT) cylinders must be installed above ground.   Governing rules are the National Propane Gas Association (NPGA) # 412-94 and the National Fire Protection Association (NFPA)-58.  The tank must be inspected by the Building Inspector prior to installation.  The placement of Anode Bags close to a tank is highly recommended.



d.
Tanks XE "tanks"  shall be installed in compliance with applicable Governmental XE "Governmental"  Requirements.



e.
No water and sanitary sewer lines shall be located within five (5) feet of a Tank XE "tanks" .


7.
The Lot Owner XE "lot owner"  shall be required to clean up any leakage from a Tank XE "tanks"  and shall be liable to the Association XE "Association"  and other Lot Owners for any damage XE "damage"  to the Lake, Association property or any Lot Owners’ Lots caused by a leaking Tank. Failure to comply with Beaver Lake requirements or Governmental XE "Governmental"  Requirements applicable to Tanks will result in the fine set forth in the Beaver Lake liquidated damages schedule.




