	BEAVER LAKE ASSOCIATION

DOCUMENT CONTROL FORM

	Requester:  Building Inspector Ron Reineke
	Ctrl Number:   095
	Date 06/28/06

	Document and Section Affected:  Building Codes  Section  III     


	Requested Change(s) (list paragraph, page, line, and change):  

G.   Erosion Control, Paragraph  3, add a second sentence to read:  “All silt fences must have a UV resistance strength retention of 80% after 500 hrs. and a tensile strength of 125lbs wrap x 110 fill.  Steel T posts are required every 6ft to 8ft with the silt fence attached to them with plastic pull straps or wire with ends bent over so as not to be a hazard.  Steel post are to be installed on the (lower side) of fence.  A flap of at least 12 inches on the bottom of the fence must face up hill and must be trenched in or at a minimum, be covered with compacted soil.

	Justification:  Why is this change needed?

Silt fence with wood stakes are not holding up during heavy rains.

	Impacts:  If not approved, what are the consequences?

When light duty fence gives away, excess soil washes into the lake


	Appropriate Committee:   None  Req  Approve __Disapprove: __N/A:  Date:   

	Recommendations for the Board:



	Approval Status:     Approved: __ __  Disapproved: ____          Date:  August 17,2006


	Board Comments:



