	BEAVER LAKE ASSOCIATION

DOCUMENT CONTROL FORM

	Requester: Appeals committee
	Ctrl Number:
120
	Date
02/2008

	Document and Section Affected:      Beaver Lake Handbook section: III. Building Code  F ,4


	Requested Change(s) (list paragraph, page, line, and change):
4.  All setback XE "setback"  measurements shall be made perpendicular from the Dwelling XE "dwelling"  or structure.

A setback XE "setback"  is normally measured to the foundation XE "foundation"  wall; however, decks XE "decks"  are measured to the maximum extremity of the deck flooring as projected to ground level.  This restriction applies to all decks attached to the main structure and to all detached XE "detached"  structures XE "structures"  such as garages XE "garages" , gazebos XE "gazebos" , etc.  Refer also to paragraph c.15.i in this section.

Change
All setback XE "setback"  measurements shall be made perpendicular from the Dwelling XE "dwelling"  or structure.

A setback XE "setback"  is normally measured to the foundation XE "foundation"  wall; floor decking of a house can not cantilever into setback area. Windows and Fireplaces that do not require footings can extend 2ft.into setback same as Soffits. Decks XE "decks"  are measured to the maximum extremity of the deck flooring as projected to ground level.  This restriction applies to all decks attached to the main structure and to all detached XE "detached"  structures XE "structures"  such as garages XE "garages" , gazebos XE "gazebos" , etc.  Refer also to paragraph C.15.i in this section.



	Justification:  Why is this change needed    Bay windows, built out windows  and fireplaces could have a problem if not exempt from rule

	Impacts:  If not approved, what are the consequences?
A house could be cantilevered over the foundation two or three feet into set back area.


	Appropriate Committee:   Appeals :    X Approve __Disapprove: __N/A:  Date:

	Recommendations for the Board:



	Approval Status:     Approved: __X __  Disapproved: ____          Date:03/20/08

	


