	BEAVER LAKE ASSOCIATION

DOCUMENT CONTROL FORM

	Requester: Board President
	Ctrl Number: 139

	Date:  July 29, 2009

	Document and Section Affected:

Beaver Lake Handbook  Section  III  Building codes   J. Detached Garages   


	Requested Change(s) (list paragraph, page, line, and change)  
Beaver Lake Handbook  Section  III  Building codes   J.  Detached Garages.
Change to   J.   Garages
And number  4. under  J.  Garages      
 4.
All garages XE "garages"  must have a concrete XE "concrete"  pad immediately in front extending the entire width of the garage and at least 20’ in depth to the garage.  All detached garages must have a concrete pad immediately in front and extending the entire width of the garage doors plus an additional eighteen inches on each side.  The concrete pad must also have a minimum depth of 20’ to the garage.

CHANGE TO

4.
All attached garages XE "garages"  must have a concrete XE "concrete"  pad immediately in front extending the entire width of the garage and at least 20’ in depth to the garage.  All detached garages must have a concrete pad immediately in front and extending the entire width of the garage doors plus an additional eighteen inches on each side.  The concrete pad must also have a minimum depth of 20’ to the garage.



	Justification:  Why is this change needed 
This will alleviate the problem of where to fined attached garages in the handbook.          


	Impacts:  If not approved, what are the consequences? Confusion on this issue will continue


	Appropriate Committee:   Approve __Disapprove: __N/A:  Date:   

	Recommendations for the Board:



	Approval Status:     Approved: __X __  Disapproved: ____          Date:  9-17-09

	


