	BEAVER LAKE ASSOCIATION

DOCUMENT CONTROL FORM

	Requester:  Board President
	Ctrl Number:  193

	Date:  1-11-13

	Document and Section Affected:      III Building Code  J  Garages  4


	Requested Change(s) (list paragraph, page, line, and change)  
From:

4.
All attached garages XE "garages"  must have a concrete XE "concrete"  pad immediately in front extending the entire width of the garage and at least 20’ in depth to the garage.  All detached garages must have a concrete pad immediately in front and extending the entire width of the garage doors plus an additional eighteen inches on each side.  The concrete pad must also have a minimum depth of 20’ to the garage.
To:

4.
All attached garages XE "garages"  must have a concrete XE "concrete"  pad immediately in front extending the entire width of the garage. The driveway must extend to the street.  
 Add:       
      5.   All detached garages (accessory buildings that have access to the street) must have a concrete pad immediately in front and extend the entire width of the garage doors plus an additional eighteen inches on each side.  The concrete pad must have a minimum depth of 20’ to the garage. Driveway from pad to street must be at a minimum sufficiently rocked as not to allow mud to be carried to street. 


	Justification:  Why is this change needed     

All Beaver Lake roads are now paved. This updates the Handbook to require that concrete driveways from a house extend to the street, standardizing appearances. 


	Impacts:  If not approved, what are the consequences? 
Some houses will be built with gravel drives that allow gravel to spread onto the paved road


	Appropriate Committee:   N/A      Approve __Disapprove: __N/A:  Date: 

	Recommendations for the Board:



	Approval Status:     Approved: __X__  Disapproved: ____          Date:  1-17-13

	Approved as recorded at 1-17-13 BOD Meeting

Updated handbook:  1-22-13  (jjp)



