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	[bookmark: _GoBack]Requester:  Russ Parmer, Board Member
	Ctrl Number: 248

	Date: 11-10-17

	Document and Section Affected:      
       Beaver Lake Handbook, Sec V. (Lake Rules and Regulations), Paragraph C. (Boat Regulations) Item 20, 21.                  


	Requested Change(s) (list paragraph, page, line, and change)  
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 Size Limits Effective 18 March 1995, excluding swim platforms at the rear of the boat.

Current SECTION V, C, 21:
Boat lengths do not include swim platforms whether it is separately attached or molded into the boat.  For boats with molded platforms, the boat length will be determined as follows:

Change to read:
20: Size limits effective December 1 2017, excluding swim platforms at the rear of the boat, will include a maximum weight of under 8800 lbs.  Boats previously registered that correctly meet the length limits but exceed the weight limits prior to December 2017 will be grandfathered under the current ownership. 
21: Boat weight is based on manufacturer specifications for hull dry weight plus maximum water ballast weight plus person/gear maximum weight.  Additionally, add on water ballasts that would cause the boat to exceed the boats manufacturer’s maximum capacity, designed to increase a boats ability to create a larger wave are prohibited. Boat lengths will be determined by manufacturer specifications.  If manufacturer specs can’t be obtained then the boat length will be determined by measuring from bow tip to the transom at the point farthest from the bow.  Boat length does not include the swim platform whether it is separately attached or molded into the boat.  For boats with molded platforms, the boat length will be determined by manufacturer specifications or if not available as follows:

	Justification:  Why is this change needed
The maximum boat lengths originally established were meant to protect our 325-acre lake from erosion, protect association members property, and maximize the number of members able to utilize the lake at the same time.  In 1995 the last time section C, 20-21 was changed a 22’ runabout would weigh less than 4,000 lbs (Hull dry weight + Gear/person max capacity). In 2017 a wake/surf boat that is 22’ or less can seat 16 and weigh over 12,000 lbs (Hull+Balast+Person/Gear).   

	Impacts:  If not approved, what are the consequences? 

Boats that routinely weigh more than 4 tons will become more numerous which in turn will increase shore erosion, shorten the lakes useful life, increase the probability of damage to members property, and decrease the number of association members that can use the lake concurrently. Manufacturer specifications provide a consistent method for members to use determining if a boat is legal for use on Beaver Lake before purchase and minimizes the need to have security measure a boat to determine legality.   
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