	BEAVER LAKE ASSOCIATION

DOCUMENT CONTROL FORM

	Requestor: BLA Board of Directors

	Ctrl Number: 217
	Date: 9-18-14

	Document and Section Affected: BLA Handbook, Section III, G. Erosion Control, 6. a.

	Requested Change(s) (list paragraph, page, line, and change):  pg. 39
From:
  6.a.  Culverts shall be constructed in such a manner as not to obstruct the natural flow of water in ditches, be no smaller than 12" in diameter and have a maximum length of 35'.  All culverts must be no closer than 5' from side property line.

To:

  6.a.  Culverts shall be constructed in such a manner as to not obstruct the natural flow of water in ditches, be no smaller than 12 inches in diameter, have a maximum length of 35 feet per driveway and have a minimum of 10 feet between culverts.  All culverts must be no closer than 5 feet from the side property line.



	Justification:  Why is this change needed?  
Handbook can be interpreted to say that 35 feet is maximum length of culvert per lot.  Large lots could have only one 35 foot driveway.


	Impacts:  If not approved, what are the consequences? 
It would not allow for a second detached garage with a driveway.


	Appropriate Committee:     Approve ____  Disapprove: ____      N/A:  X      Date: 9-18-14

	Recommendations for the Board:


	Approval Status:     Approved: __X__  Disapproved: ____          Date:  9-18-14

	Board Comments:

Approved as recorded at 09-18-14 BOD Meeting

Updated handbook:  09-23-14 (jjp)



