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DOCUMENT CONTROL FORM

	Requestor: Dave Hibler
	Ctrl Number: 332
	Date: 9-15-2023

	[bookmark: _Toc89994933][bookmark: _Toc225764775]Document and Section Affected: 
Handbook Section III: Building Codes; F; 4


	Requested Change(s) (list paragraph, page, line, and change):  
From: All setback measurements shall be made perpendicular from the Dwelling or structure. A setback is normally measured to the foundation wall; floor decking of a house cannot cantilever into setback area. Windows and Fireplaces that do not require footings can extend 2 feet into setback same as Soffits. Decks are measured to the maximum extremity of the deck flooring as projected to ground level.  This restriction applies to all decks attached to the main structure and to all detached structures such as garages, gazebos, etc.  Refer also to paragraph III.C.15.i

To: All setback measurements shall be made perpendicular from the Dwelling or structure. A setback is normally measured to the foundation wall; floor decking of a house cannot cantilever into setback area. Windows and Fireplaces that do not require footings can extend 2 feet into setback same as Soffits. Decks are measured to the maximum extremity of the deck structure as projected to ground level.  This restriction applies to all decks attached to the main structure and to all detached structures such as garages, gazebos, etc.  Refer also to paragraph III.C.15.i
 

	Justification:  Why is this change needed?  
Clear up verbiage because the flooring isn’t the furthest point of a deck.


	Impacts:  If not approved, what are the consequences?  
Leaves a loophole for decks in setback area.


	Appropriate Committee:     Approve ____  Disapprove: ____      N/A:__X__     Date:

	Recommendations for the Board:
Committee:
Board:


	Approval Status:     Approved: _X_  Disapproved: ____          Date:  9-21-23

	Board Comments:
Approved as recorded at the 9-21-23 BOD Meeting
Updated Handbook:  11-1-23 (jjp)





