	BEAVER LAKE ASSOCIATION

DOCUMENT CONTROL FORM

	Requester:  Ron Reineke

	Ctrl Number:
063
	Date:  12 Nov 04

	Document and Section Affected:
Handbook, Section III, Building Code

	Requested Change(s) (list paragraph, page, line, and change):

Add a new paragraph C.15.i to read: 

“Overhangs, except for soffits and porches as identified in paragraph F.4, shall not protrude into any setback  without a variance.  Soffits may extend into the setback by no more than 2’.”

	Justification:  Why is this change needed?

Setbacks are currently measured from the foundation.  Overhangs have been allowed to protrude into the setback but some people are abusing the rule.  There is a shed just west and up the hill of the stop sign joining Beaver Lake Blvd and Elk Lane (Northwest end of the lake) which meets the 30’ setback but the overhang is at least 5’.  Its sort of like a porch without support poles.  This loophole needs to be closed to prevent this sort of thing.  Just wait for the poles to be installed.  Recommend not allowing overhangs to go inside of setback without a variance with the exception of soffits with a maximum hang of 2' into the setback.. 



	Impacts:  If not approved, what are the consequences?

Inventive residents can extend roofs well into the easement without a vairance.



	Appropriate Committee:   Bld Insp  Approve _X___Disapprove: ____N/A: ______Date:

	Recommendations for the Board:
Approve the DCF



	Approval Status:     Approved: __X__  Disapproved: ____          Date: 18 Nov 04

	Board Comments:
18 Nov 04:  Approved at Nov Board Meeting

Incorporated on 2 Dec 04 for the Jan 05 version of the handbook.

9 May 06:  Changed “F.2.b” to read paragraph “F” to cover the entire section.  Briefed to Board. 
9 May 06:  Added a reference to PPH C.15.i in section F.4 for clarification.  Briefed to Board.



