	BEAVER LAKE ASSOCIATION

DOCUMENT CONTROL FORM

	Requester:  Rick Croasdale

	Ctrl Number:
071
	Date:  28 Dec 04

	Document and Section Affected:
Handbook, Section III, Building Code

	Requested Change(s) (list paragraph, page, line, and change):

Paragraph C.5  Add a new sub-paragraph to read:

“In addition, all Beaver Lake Association homes are recommended to have a working sewage backflow prevention device located between the main sewer line and the house according the Nebraska Uniform Plumbing Code or the owner will assume the responsibility of flood damage inside the home should there be a sewer system malfunction.  All newly constructed homes are required to have a backflow device before the house is connected to the system.”



	Justification:  Why is this change needed?

Backflow devices are required according to the Uniform Plumbing Code and it should be annotated as such in our Covenants.



	Impacts:  If not approved, what are the consequences?

Increased risk of a homeowner not knowing that backflow devices are required to save possible and extensive flood damage in case of an inadvertent liftstation malfunction.



	Appropriate Committee:   Utility  Approve _X_  Disapprove: __N/A:  Date:   4 Jan 05

	Recommendations for the Board:
Approve the DCF.



	Approval Status:     Approved: _X_  Disapproved: ____          Date:  20 Jan 2005

	Board Comments:
18 Jan 2005:  Approved at working session with minor word change.  Required is now Recommended.

20 Jan 2005:  Approved at monthly Board meeting




