	BEAVER LAKE ASSOCIATION

DOCUMENT CONTROL FORM

	Requestor:  Board

	Ctrl Number:  174
	Date:  8-18-2011

	Document and Section Affected:  Beaver Lake Handbook, Section III – Building Codes

	Requested Change(s) (list paragraph, page, line, and change):  III, G Erosion Control, 6 Culverts, a.
Change from:

6.
Culverts:  Culverts shall come under the following rules:

a.
Culverts shall be constructed in such a manner as not to obstruct the natural flow of water in ditches, be no smaller than 12" in diameter and have a maximum length of 30'.  All culverts must be no closer than 5' from side property line.

Change to:

6.
Culverts:  Culverts shall come under the following rules:

a.
Culverts shall be constructed in such a manner as not to obstruct the natural flow of water in ditches, be no smaller than 12" in diameter and have a maximum length of 35'.  All culverts must be no closer than 5' from side property line.



	Justification:  Why is this change needed?

Driveways without culverts can have as wide of driveway as they want to build.

	Impacts:  If not approved, what are the consequences?

Confusion over how wide of a driveway a residence can have.


	Appropriate Committee:     Approve ____  Disapprove: ____      N/A:__X__       Date:

	Recommendations for the Board



	Approval Status:     Approved: __X__  Disapproved: ____          Date:  8-18-11

	Board Comments:

Approved as recorded at 8-18-11 BOD Meeting

Updated handbook:  8-30-11 (jjp)



