	BEAVER LAKE ASSOCIATION

DOCUMENT CONTROL FORM

	Requester:  Board President
	Ctrl Number:  188

	Date:  1-11-13

	Document and Section Affected:      III Building codes H Dwellings  7


	   Requested Change(s) (list paragraph, page, line, and change)  
FROM:

7.
For safety purposes, there must be a landing XE "landing"  for every story of a stairway leading to above-ground level entryways XE "entryways" , porches XE "porches" , verandas XE "verandas" , or decks XE "decks" .  In addition, there must be a landing at the top of such stairway which is at least ten (10) feet by twelve (12) feet.
TO:

7.
For safety purposes, there must be a landing (a minimum size of four feet by four feet) XE "landing"  for every story of a stairway leading to above-ground level entryways XE "entryways" , porches XE "porches" , verandas XE "verandas" , or decks XE "decks" .  In addition, there must be a deck at the top of such stairway which is at least six (6) feet by eight (8) feet.



	Justification:  Why is this change needed 

To clarify what is meant by a landing 


	Impacts:  If not approved, what are the consequences?
Confusion on what a landing is


	Appropriate Committee:   N/A      Approve __Disapprove: __N/A:  Date:

	Recommendations for the Board:



	Approval Status:     Approved: __X__  Disapproved: ____          Date:  1-17-13

	Approved as recorded at 1-17-13 BOD Meeting

Updated handbook:  1-22-13  (jjp)



