	BEAVER LAKE ASSOCIATION

DOCUMENT CONTROL FORM

	Requestor: Troy Weatherby & Jim Wieringa
	Ctrl Number: 249 
	Date: 12-1-17

	Document and Section Affected: Beaver Lake Handbook, Section III Building Codes, Subsection H, Paragraph #8

	Requested Change(s) (list paragraph, page, line, and change): 
From: 8.  Except for Mobile homes, all dwellings must have a 2 car wide, attached garage unless it can be demonstrated that such garage will cause undue hardship to the lot owner or will not fit within the prescribed setbacks.  In that case, a 2 car wide, detached XE "detached"  garage will be required.
To: 8.
Except for Mobile homes, all dwellings must have a minimum of a 2 car wide, attached garage unless it can be demonstrated that such garage will cause undue hardship to the lot owner or will not fit within the prescribed setbacks.  In that case, a 2 car wide, detached XE "detached"  garage will be required. (2 cars wide is defined as, a garage door with a minimum width of 16’ or 2 garage doors with a minimum of 9’ width each).

	Justification:  Why is this change needed?  To clarify what a 2 car wide garage is expected to be.


	Impacts:  If not approved, what are the consequences? Assumptions will be made that an 8’ wide door could be used, if you can park the cars in tandem or any number of arrangements.


	Appropriate Committee:     Approve ____  Disapprove: ____      N/A:____     Date:

	Recommendations for the Board: Review and approve


	Approval Status:     Approved: __X__  Disapproved: ____          Date: 12-21-17

	Board Comments:

Approved as recorded at 12-21-17 BOD Meeting

Updated Handbook:  1-5-18 (jjp)




