	BEAVER LAKE ASSOCIATION

DOCUMENT CONTROL FORM

	Requestor: Troy Weatherby / JimWieringa
	Ctrl Number: 251 
	Date: 1-31-18

	Document and Section Affected: Handbook, Section III Building Codes, Subsection P, #4

	Requested Change(s) (list paragraph, page, line, and change): 
From: 4.
Above-ground Tanks XE "tanks"  located on a Residential XE "residential"  Lot, Equestrian XE "equestrian"  Lot, Mobile Home XE "mobile home"  Lot, or Commercial XE "commercial"  Lot shall be screened from view by shrubbery XE "shrubbery"  or a solid wood or plastic fence XE "fence" .  Chain link fences XE "fences"  are not permitted to screen a Tank.  If wood or plastic lattice is used to screen a Tank, the holes in such lattice may not exceed one inch (1) inch square (one and one-half (1½ ) inches when measured diagonally.   Shrubbery used to screen a Tank shall be of the evergreen family and shall be large and dense enough when planted to completely shield the Tank from view.  In screening a Tank, consideration should be given to proper ventilation and access for refilling and repair XE "repair" .

To: 4.
Above-ground propane tanks XE "tanks"  located on a Residential XE "residential"  Lot, Equestrian XE "equestrian"  Lot, Mobile Home XE "mobile home"  Lot, or Commercial XE "commercial"  Lot shall be screened from view by a solid wood or plastic fence or a fence that appears to be solid to the view XE "fence" . The fence shall have an opening of 6” between the ground and the bottom of the fence to allow gas to escape during filling. The fence shall also have an area low enough to allow for filling the tank and still shield the tank from view or a gate for filling the tank. Drawings and specifications must be submitted to the Building Inspector to obtain a permit prior to construction. Contact your propane supplier prior to the fence installation for supply line locates and recommendations. 


	Justification:  Why is this change needed?  Eliminate the use of lattice due to its lack of strength and the visibility of through the panel. Also eliminate shrubbery due to its interference with the tank as it grows due to the lack of maintenance. If a tank is to screened from view it should be done properly.


	Impacts:  If not approved, what are the consequences? Materials are being used that do not screen the tank from view and shrubbery is an ongoing problem due to growth and roots around the supply lines. 


	Appropriate Committee:     Approve ____  Disapprove: ____      N/A:__X__     Date:

	Recommendations for the Board: Review and approve


	Approval Status:     Approved: __X__  Disapproved: ____          Date: 3-15-18

	Board Comments:

Approved as recorded at 3-15-18 BOD Meeting

Updated Handbook:  4-5-18 (jjp)




