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From:

 L.
BOAT DOCKS AND BOAT SLIPS


1.
A Beaver Lake Building Permit XE "building permit"  shall be obtained from the Building Inspector XE "Building Inspector"  before construction of any Boat XE "boat"  Dock XE "dock"  or Boat Slip XE "slip" .


2.
A dock shall be constructed so as not to excessively hinder inspection or repair XE "repair"  of shoreline XE "shoreline" .

3.
A Boat XE "boat"  Dock XE "dock"  shall extend no more than twenty-four (24) feet in length over the water from the shoreline XE "shoreline" .  Boat Docks in coves require Board approval due to limited shoreline and lake area access in coves.


4.
A Boat XE "boat"  Dock XE "dock"  or Boat Slip XE "slip"  shall be placed no closer than ten (10) feet to the boundary line with the adjoining Lot.


5.
A railing on a Boat XE "boat"  Dock XE "dock"  or temporary dock is permitted but may not exceed three (3) feet in height. 


6.
Unless there is a Dwelling XE "dwelling" , a functional boat ramp must be no closer than 5’ from the lot line and no wider than 8’. There are no restrictions for boat ramps XE "ramps"  on lots with a dwelling. Applications for permits must be accompanied with a letter showing approval of abutting Lot Owners XE "lot owner" .


7.
Boat XE "boat"  Docks shall be constructed in such a manner as to not hinder the flow of traffic in a cove or elsewhere on the Lake.


8a.     Boat XE "boat"  Docks, Boat Slips and boatlifts shall be maintained in good repair XE "repair"  in order to preserve the beauty of the Subdivision.  If this policy is violated, the Association XE "Association"  at its sole discretion may initiate action to repair or remove the structure at owner’s expense.


8b.    Boat lifts, excluding canopies, shall not be positioned more than 30feet from the existing 1050ft. elevation at the shoreline unless explicitly approved by the Board of Directors (BOD) or the BOD agent as the only reasonable option available.


9.      Permanent Boat XE "boat"  Docks built by private Lot Owners XE "lot owner"  shall not be built on Association XE "Association"  access areas unless approved by the Board of Directors XE "Board of Directors" .  Such permanent Boat Docks shall become the property of the Association.

TO: 
L.
BOAT DOCKS, SLIPS, RAMPS, and LIFTS


1.
A Beaver Lake Building Permit XE "building permit"  shall be obtained from the Building Inspector XE "Building Inspector"  before construction or placement of any Boat XE "boat"  Dock, XE "dock"  Boat Slip XE "slip" , Boat Ramp, or Boat Lift.


2.
A dock shall be constructed so as not to excessively hinder inspection or repair XE "repair"  of shoreline XE "shoreline" .

3.
A Boat XE "boat"  Dock XE "dock"  shall extend no more than twenty-four (24) feet in length over the water from the shoreline XE "shoreline" .  Boat Docks in coves require Board approval due to limited shoreline and lake area access in coves.


4.
A boat XE "boat"  dock XE "dock"  or Boat Slip XE "slip"  shall be placed no closer than ten (10) feet to the boundary line with the adjoining Lot.


5.
A railing on a boat XE "boat"  dock XE "dock"  or temporary dock is permitted but may not exceed three (3) feet in height. 


6.
Unless there is a dwelling XE "dwelling" , a functional boat ramp must be no closer than 5’ from the lot line and no wider than 8’. There are no restrictions for boat ramps XE "ramps"  on lots with a dwelling. Applications for permits must be accompanied with a letter showing approval of abutting Lot Owners XE "lot owner" .


7.
Boat XE "boat"  Docks shall be constructed in such a manner as to not hinder the flow of traffic in a cove or elsewhere on the Lake.

          8.       Permanent Boat XE "boat"  Docks built by private Lot Owners XE "lot owner"  shall not be built on Association XE "Association"  access areas unless approved by the Board of Directors XE "Board of Directors" .  Such permanent Boat Docks shall become the property of the Association.
          9.a.  Boat XE "boat"  docks, boat slips and boat lifts shall be maintained in good repair XE "repair"  in order to preserve the beauty of the Subdivision.  If this policy is violated, the Association XE "Association"  at its sole discretion may initiate action to repair or remove the structure at owner’s expense.

         9b.      Boat lifts, excluding canopies, shall not be positioned more than 30 feet from the existing 1050 ft. elevation at the shoreline unless explicitly approved by the Board of Directors (BOD) or the BOD agent as the only reasonable option available.

         9c.      All boat lifts shall be of the portable type with no permanent attachment to the lake bed on which it rests.

         9d.     There shall be no permanent roof structures attached to the boat lift with the exception of canopies and canopy frames.   



	Justification:  Why is this change needed?  To give better guidance to property owners about boat lifts.


	Impacts:  If not approved, what are the consequences? 
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